#

##

##

##

##

##

    礦ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.14.0.0
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: lzb lzb, lzb, LIC=EPPDY-I883H-5AJDF-6A3NP-H8EHC-WXFJU

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.14.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.05 update 1 (build 106)
    Assembler:       Armasm.exe V5.05 update 1 (build 106)
    Linker/Locator:  ArmLink.exe V5.05 update 1 (build 106)
    Library Manager: ArmAr.exe V5.05 update 1 (build 106)
    Hex Converter:   FromElf.exe V5.05 update 1 (build 106)
    CPU DLL:         SARMCM3.DLL V5.14.0.0
    Dialog DLL:      DCM.DLL V1.13.1.0
    Target DLL:      STLink\ST-LINKIII-KEIL_SWO.dll V2.0.14.0_KEIL
    Dialog DLL:      TCM.DLL V1.14.4.0

    Project:
    C:\Users\Administrator\Desktop\IDT\软件部分\代码\智能盆栽\USER\Template.uvprojx
    Project File Date:  01/08/2019

    Output:
    Build target 'Template'
    compiling main.c...
    main.c(43): warning:  #1035-D: single-precision operand implicitly converted to double-precision
                            total_water = total_water+0.5*Liquid_dat;
    main.c(20): warning:  #550-D: variable "luxfloat" was set but never used
        u8 luxfloat;//小数部分
    main.c: 2 warnings, 0 errors
    linking...
    Program Size: Code=8428 RO-data=424 RW-data=48 ZI-data=1896
    FromELF: creating hex file...
    "..\OBJ\Template.axf" - 0 Error(s), 2 Warning(s).

    Collection of Component include folders:
      C:\Users\Administrator\Desktop\IDT\软件部分\代码\智能盆栽\USER\RTE
      C:\Keil_v5\ARM\PACK\Keil\STM32F4xx_DFP\1.0.8\Device\Include

    Collection of Component Files used: