#

##

##

    礦ision Build Log
    Project:
    F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\Project.uvproj
    Project File Date:  01/01/2011

    Output:
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    ..\spi.h(25): warning:  #47-D: incompatible redefinition of macro "SPI2_MISO" (declared at line 19)
    ..\spi.h:   #define SPI2_MISO      GPIO_Pin_6
    ..\spi.h:           ^
    ..\spi.h(26): warning:  #47-D: incompatible redefinition of macro "SPI2_MOSI" (declared at line 20)
    ..\spi.h:   #define SPI2_MOSI      GPIO_Pin_7
    ..\spi.h:           ^
    ..\spi.h: ..\main.c: 2 warnings, 0 errors
    compiling spi.c...
    ..\spi.h(25): warning:  #47-D: incompatible redefinition of macro "SPI2_MISO" (declared at line 19)
    ..\spi.h:   #define SPI2_MISO      GPIO_Pin_6
    ..\spi.h:           ^
    ..\spi.h(26): warning:  #47-D: incompatible redefinition of macro "SPI2_MOSI" (declared at line 20)
    ..\spi.h:   #define SPI2_MOSI      GPIO_Pin_7
    ..\spi.h:           ^
    ..\spi.c(48): error:  #20: identifier "RCC_APB1Periph_SPI1" is undefined
    ..\spi.c:       RCC_APB1PeriphClockCmd( RCC_APB1Periph_SPI1, ENABLE );
    ..\spi.c:                               ^
    ..\spi.c(53): error:  #20: identifier "SPI1_MISO" is undefined
    ..\spi.c:       GPIO_InitStructure.GPIO_Pin = SPI1_MISO| SPI1_MOSI| SPI1_SCK;
    ..\spi.c:                                     ^
    ..\spi.c(53): error:  #20: identifier "SPI1_MOSI" is undefined
    ..\spi.c:       GPIO_InitStructure.GPIO_Pin = SPI1_MISO| SPI1_MOSI| SPI1_SCK;
    ..\spi.c:                                                ^
    ..\spi.c: ..\spi.c: 2 warnings, 3 errors
    compiling delay.c...
    compiling NRF24L01.c...
    ..\spi.h(25): warning:  #47-D: incompatible redefinition of macro "SPI2_MISO" (declared at line 19)
    ..\spi.h:   #define SPI2_MISO      GPIO_Pin_6
    ..\spi.h:           ^
    ..\spi.h(26): warning:  #47-D: incompatible redefinition of macro "SPI2_MOSI" (declared at line 20)
    ..\spi.h:   #define SPI2_MOSI      GPIO_Pin_7
    ..\spi.h:           ^
    ..\spi.h: ..\NRF24L01.c: 2 warnings, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    Target not created
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    .\神舟III号\24G无线通信实验.axf: Error: L6218E: Undefined symbol SPI2_Init (referred from nrf24l01.o).
    .\神舟III号\24G无线通信实验.axf: Not enough information to list image symbols.
    .\神舟III号\24G无线通信实验.axf: Finished: 1 information, 0 warning and 1 error messages.
    Target not created
    Build target '神舟III号'
    compiling spi.c...
    linking...
    Program Size: Code=4008 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4008 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Build target '神舟III号'
    compiling main.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    linking...
    .\神舟III号\24G无线通信实验.axf: Error: L6218E: Undefined symbol SPI1_Init (referred from nrf24l01.o).
    .\神舟III号\24G无线通信实验.axf: Not enough information to list image symbols.
    .\神舟III号\24G无线通信实验.axf: Finished: 1 information, 0 warning and 1 error messages.
    Target not created
    Build target '神舟III号'
    compiling spi.c...
    compiling NRF24L01.c...
    linking...
    .\神舟III号\24G无线通信实验.axf: Error: L6218E: Undefined symbol SPI2_Init (referred from nrf24l01.o).
    .\神舟III号\24G无线通信实验.axf: Not enough information to list image symbols.
    .\神舟III号\24G无线通信实验.axf: Finished: 1 information, 0 warning and 1 error messages.
    Target not created
    Build target '神舟III号'
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    linking...
    Program Size: Code=4000 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4000 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4000 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    **JLink Warning: No matching core found.
    ***JLink Error: Supply voltage too low (1 Volt is required, Measured: 0.0 Volt).
    Please check target power.
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling main.c...
    compiling stm32_eval.c...
    linking...
    Program Size: Code=4000 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4000 RO-data=516 RW-data=104 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    linking...
    Program Size: Code=4092 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling main.c...
    compiling stm32_eval.c...
    linking...
    Program Size: Code=4092 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4092 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(39): warning:  #223-D: function "SPI1_Init" declared implicitly
    ..\NRF24L01.c:          SPI1_Init();                                       //初始化SPI
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c: ..\NRF24L01.c: 1 warning, 0 errors
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4092 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 1 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    **JLink Warning: No matching core found.
    ***JLink Error: Supply voltage too low (1 Volt is required, Measured: 0.0 Volt).
    Please check target power.
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 3.325V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling spi.c...
    linking...
    .\神舟III号\24G无线通信实验.axf: Error: L6218E: Undefined symbol SPI2_ReadWriteByte (referred from nrf24l01.o).
    .\神舟III号\24G无线通信实验.axf: Not enough information to list image symbols.
    .\神舟III号\24G无线通信实验.axf: Finished: 1 information, 0 warning and 1 error messages.
    Target not created
    Build target '神舟III号'
    compiling main.c...
    compiling spi.c...
    compiling NRF24L01.c...
    ..\NRF24L01.c(61): warning:  #223-D: function "SPI2_ReadWriteByte" declared implicitly
    ..\NRF24L01.c:          status =SPI2_ReadWriteByte(regaddr); //发送寄存器号
    ..\NRF24L01.c:                  ^
    ..\NRF24L01.c(71): warning:  #223-D: function "SPI2_ReadWriteByte" declared implicitly
    ..\NRF24L01.c:          SPI2_ReadWriteByte(regaddr);     //发送寄存器号
    ..\NRF24L01.c:          ^
    ..\NRF24L01.c(83): warning:  #223-D: function "SPI2_ReadWriteByte" declared implicitly
    ..\NRF24L01.c:          status=SPI2_ReadWriteByte(regaddr);   //发送寄存器值(位置),并读取状态值
    ..\NRF24L01.c:                 ^
    ..\NRF24L01.c(95): warning:  #223-D: function "SPI2_ReadWriteByte" declared implicitly
    ..\NRF24L01.c:          status = SPI2_ReadWriteByte(regaddr);                //发送寄存器值(位置),并读取状态值
    ..\NRF24L01.c:                   ^
    ..\NRF24L01.c: ..\NRF24L01.c: 4 warnings, 0 errors
    linking...
    .\神舟III号\24G无线通信实验.axf: Error: L6218E: Undefined symbol SPI2_ReadWriteByte (referred from nrf24l01.o).
    .\神舟III号\24G无线通信实验.axf: Not enough information to list image symbols.
    .\神舟III号\24G无线通信实验.axf: Finished: 1 information, 0 warning and 1 error messages.
    Target not created
    Build target '神舟III号'
    compiling NRF24L01.c...
    linking...
    Program Size: Code=4012 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4012 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling main.c...
    compiling spi.c...
    compiling NRF24L01.c...
    linking...
    Program Size: Code=4012 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4012 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4012 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=4016 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=3992 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    **JLink Warning: No matching core found.
    ***JLink Error: Supply voltage too low (1 Volt is required, Measured: 0.0 Volt).
    Please check target power.
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.325V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=3992 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Build target '神舟III号'
    compiling stm32f10x_it.c...
    compiling main.c...
    compiling spi.c...
    compiling delay.c...
    compiling NRF24L01.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_gpio.c...
    compiling misc.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_i2c.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling stm32_eval.c...
    assembling startup_stm32f10x_hd.s...
    linking...
    Program Size: Code=3992 RO-data=432 RW-data=72 ZI-data=1040
    FromELF: creating hex file...
    ".\神舟III号\24G无线通信实验.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\光盘资料\\wuxaian\\STM32F10x_StdPeriph_Lib_V3.3.0\\project\\16.2.4G无线通信实验（神舟III号）\\MDK-ARM\\神舟III号\\24G无线通信实验.AXF"
    Set JLink Project File to "F:\光盘资料\wuxaian\STM32F10x_StdPeriph_Lib_V3.3.0\project\16.2.4G无线通信实验（神舟III号）\MDK-ARM\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F107VC
    VTarget = 3.332V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.