# Static Call Graph for image ..\OBJ\GSM.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 24]: Last Updated: Fri Jul 24 17:27:17 2015

### Maximum Stack Usage = 344 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- LCD_Fill ⇒ LCD_Fill

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CTP_Scan from ott2001a.o(.text) referenced from touch.o(.text)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from usart3.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from usart2.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TP_Adjust from touch.o(.text) referenced 2 times from touch.o(.data)
  - TP_Init from touch.o(.text) referenced 2 times from touch.o(.data)
  - TP_Scan from touch.o(.text) referenced 2 times from touch.o(.data)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from usart2.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from usart3.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - _get_lc_ctype from lc_ctype_c.o(locale$$code) referenced from rt_ctype_table.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - _sputc from _sputc.o(.text) referenced 2 times from c89vsprintf.o(.text)
  - fputc from usart.o(.text) referenced from _printf_char_file.o(.text)
  - mem_init from malloc.o(.text) referenced 2 times from malloc.o(.data)
  - mem_perused from malloc.o(.text) referenced 2 times from malloc.o(.data)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 90 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __decompress1 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_n (Thumb, 0 bytes, Stack size unknown bytes, _printf_n.o(.ARM.Collect$$_printf_percent$$00000001))
  [Calls]

  - >> _printf_charcount

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_p (Thumb, 0 bytes, Stack size unknown bytes, _printf_p.o(.ARM.Collect$$_printf_percent$$00000002))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_p ⇒ _printf_hex_ptr ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_hex_ptr

  _printf_f (Thumb, 0 bytes, Stack size unknown bytes, _printf_f.o(.ARM.Collect$$_printf_percent$$00000003))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_f ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_e (Thumb, 0 bytes, Stack size unknown bytes, _printf_e.o(.ARM.Collect$$_printf_percent$$00000004))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_e ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_g (Thumb, 0 bytes, Stack size unknown bytes, _printf_g.o(.ARM.Collect$$_printf_percent$$00000005))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_g ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_a (Thumb, 0 bytes, Stack size unknown bytes, _printf_a.o(.ARM.Collect$$_printf_percent$$00000006))

  _printf_ll (Thumb, 0 bytes, Stack size unknown bytes, _printf_ll.o(.ARM.Collect$$_printf_percent$$00000007))

  _printf_i (Thumb, 0 bytes, Stack size unknown bytes, _printf_i.o(.ARM.Collect$$_printf_percent$$00000008))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_i ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_u (Thumb, 0 bytes, Stack size unknown bytes, _printf_u.o(.ARM.Collect$$_printf_percent$$0000000A))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_u ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_o (Thumb, 0 bytes, Stack size unknown bytes, _printf_o.o(.ARM.Collect$$_printf_percent$$0000000B))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_o ⇒ _printf_int_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_oct

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_lli (Thumb, 0 bytes, Stack size unknown bytes, _printf_lli.o(.ARM.Collect$$_printf_percent$$0000000D))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_lli ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_lld (Thumb, 0 bytes, Stack size unknown bytes, _printf_lld.o(.ARM.Collect$$_printf_percent$$0000000E))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_lld ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_llu (Thumb, 0 bytes, Stack size unknown bytes, _printf_llu.o(.ARM.Collect$$_printf_percent$$0000000F))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_llu ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_llo (Thumb, 0 bytes, Stack size unknown bytes, _printf_llo.o(.ARM.Collect$$_printf_percent$$00000010))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_llo ⇒ _printf_ll_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_ll_oct

  _printf_llx (Thumb, 0 bytes, Stack size unknown bytes, _printf_llx.o(.ARM.Collect$$_printf_percent$$00000011))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_llx ⇒ _printf_ll_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_ll_hex

  _printf_l (Thumb, 0 bytes, Stack size unknown bytes, _printf_l.o(.ARM.Collect$$_printf_percent$$00000012))

  _printf_c (Thumb, 0 bytes, Stack size unknown bytes, _printf_c.o(.ARM.Collect$$_printf_percent$$00000013))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_c ⇒ _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_char

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_string

  _printf_lc (Thumb, 0 bytes, Stack size unknown bytes, _printf_lc.o(.ARM.Collect$$_printf_percent$$00000015))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_lc ⇒ _printf_wchar ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wchar

  _printf_ls (Thumb, 0 bytes, Stack size unknown bytes, _printf_ls.o(.ARM.Collect$$_printf_percent$$00000016))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_ls ⇒ _printf_wstring ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wstring

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_common (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))
  [Calls]

  - >> __rt_locale

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000010))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_ctype_2 ⇒ _get_lc_ctype
  [Calls]
  - >> _get_lc_ctype

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000014))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_numeric_2 ⇒ _get_lc_numeric
  [Calls]
  - >> _get_lc_numeric

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 344 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  HC05_Role_Show (Thumb, 54 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = HC05_Role_Show ⇒ HC05_Get_Role ⇒ u3_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> LCD_ShowString
  - >> HC05_Get_Role
  [Called By]
  - >> main

  HC05_Sta_Show (Thumb, 52 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = HC05_Sta_Show ⇒ LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_ShowString
  [Called By]
  - >> main

  main (Thumb, 554 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 344 + Unknown Stack Size
  - Call Chain = main ⇒ f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> uart_init
  - >> u2_printf
  - >> sim900a_test
  - >> mem_init
  - >> f_mount
  - >> exfuns_init
  - >> delay_ms
  - >> delay_init
  - >> USART2_Init
  - >> NVIC_Configuration
  - >> LED_Init
  - >> LCD_ShowString
  - >> LCD_Init
  - >> LCD_Fill
  - >> KEY_Scan
  - >> KEY_Init
  - >> HC05_Set_Cmd
  - >> HC05_Init
  - >> HC05_Get_Role
  - >> HC05_Sta_Show
  - >> HC05_Role_Show
  - >> __2sprintf
  [Called By]
  - >> __rt_entry_main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  LED_Init (Thumb, 72 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Init (Thumb, 82 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = KEY_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinRemapConfig
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Scan (Thumb, 154 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = KEY_Scan
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> main
  - >> sim900a_gprs_test
  - >> sim900a_tcpudp_test

  LCD_WR_REG (Thumb, 60 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_ReadPoint
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_ReadReg
  - >> LCD_WriteReg
  - >> LCD_Init

  LCD_WR_DATAX (Thumb, 60 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_DATAX
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_Init

  LCD_RD_DATA (Thumb, 118 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_RD_DATA
  [Calls]
  - >> delay_us
  - >> GPIO_ResetBits
  - >> GPIO_ReadInputData
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_ReadReg
  - >> LCD_Init

  LCD_WriteReg (Thumb, 68 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_WR_REG
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_SetCursor
  - >> LCD_Init

  LCD_ReadReg (Thumb, 16 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_ReadReg ⇒ LCD_RD_DATA
  [Calls]
  - >> LCD_RD_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Init

  LCD_WriteRAM_Prepare (Thumb, 12 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_WriteRAM_Prepare ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Clear
  - >> LCD_DrawPoint
  - >> LCD_Fill

  LCD_WriteRAM (Thumb, 60 bytes, Stack size 8 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> GPIO_SetBits

  LCD_BGR2RGB (Thumb, 26 bytes, Stack size 12 bytes, lcd.o(.text), UNUSED)
  [Called By]

  - >> LCD_ReadPoint

  LCD_SetCursor (Thumb, 860 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetCursor ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_WriteReg
  - >> LCD_WR_REG
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Clear
  - >> LCD_Set_Window
  - >> LCD_DrawPoint
  - >> LCD_ReadPoint
  - >> LCD_Fill

  LCD_ReadPoint (Thumb, 466 bytes, Stack size 24 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> delay_us
  - >> GPIO_ResetBits
  - >> GPIO_ReadInputData
  - >> LCD_SetCursor
  - >> LCD_BGR2RGB
  - >> LCD_WR_REG
  - >> GPIO_SetBits

  LCD_DisplayOn (Thumb, 80 bytes, Stack size 8 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_REG

  LCD_DisplayOff (Thumb, 78 bytes, Stack size 8 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_REG

  LCD_Scan_Dir (Thumb, 1516 bytes, Stack size 24 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_WriteReg
  - >> LCD_WR_REG
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_Display_Dir

  LCD_DrawPoint (Thumb, 76 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> GPIO_SetBits
  [Called By]
  - >> TP_Draw_Big_Point
  - >> TP_Drow_Touch_Point
  - >> LCD_Draw_Circle
  - >> LCD_DrawLine

  LCD_Fast_DrawPoint (Thumb, 978 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_WriteReg
  - >> LCD_WR_REG
  - >> GPIO_SetBits
  [Called By]
  - >> LCD_ShowChar
  - >> Show_Font

  LCD_Display_Dir (Thumb, 420 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_Display_Dir ⇒ LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_Scan_Dir
  [Called By]
  - >> LCD_Init

  LCD_Set_Window (Thumb, 1212 bytes, Stack size 56 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_SetCursor
  - >> LCD_WriteReg
  - >> LCD_WR_REG
  - >> GPIO_SetBits

  LCD_Clear (Thumb, 164 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_Clear ⇒ LCD_SetCursor ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> GPIO_SetBits
  [Called By]
  - >> TP_Init
  - >> TP_Adjust
  - >> LCD_Init
  - >> sim900a_mtest_ui
  - >> sim900a_gprs_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_ui
  - >> sim900a_sms_read_test
  - >> sim900a_call_test

  LCD_Init (Thumb, 14868 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = LCD_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_us
  - >> LCD_Clear
  - >> LCD_Display_Dir
  - >> LCD_ReadReg
  - >> LCD_WriteReg
  - >> LCD_RD_DATA
  - >> LCD_WR_DATAX
  - >> LCD_WR_REG
  - >> GPIO_PinRemapConfig
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> delay_ms
  - >> __2printf
  [Called By]
  - >> main

  LCD_Fill (Thumb, 226 bytes, Stack size 48 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 88 + In Cycle
  - Call Chain = LCD_Fill ⇒ LCD_Fill (Cycle)
  [Calls]
  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> GPIO_SetBits
  - >> LCD_Fill
  [Called By]
  - >> LCD_Fill
  - >> main
  - >> sim900a_gprs_test
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> sim900a_key_staset
  - >> sim900a_load_keyboard

  LCD_Color_Fill (Thumb, 140 bytes, Stack size 40 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Write
  - >> GPIO_ResetBits
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> GPIO_SetBits

  LCD_DrawLine (Thumb, 176 bytes, Stack size 72 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_DrawRectangle

  LCD_DrawRectangle (Thumb, 80 bytes, Stack size 24 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine
  [Called By]
  - >> sim900a_load_keyboard

  LCD_Draw_Circle (Thumb, 176 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_Draw_Circle ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point

  LCD_ShowChar (Thumb, 268 bytes, Stack size 40 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_Fast_DrawPoint
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum
  - >> LCD_ShowString
  - >> sim900a_call_test
  - >> Show_Str

  LCD_Pow (Thumb, 22 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Pow
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 148 bytes, Stack size 56 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_Pow
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show

  LCD_ShowxNum (Thumb, 190 bytes, Stack size 64 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_Pow
  - >> LCD_ShowChar

  LCD_ShowString (Thumb, 102 bytes, Stack size 40 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adjust
  - >> TP_Adj_Info_Show
  - >> main
  - >> HC05_Sta_Show
  - >> HC05_Role_Show

  SPI1_ReadWriteByte (Thumb, 78 bytes, Stack size 16 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI1_ReadWriteByte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> SD_SendBlock
  - >> SD_RecvData
  - >> SD_SPI_ReadWriteByte
  - >> SPI_Flash_WAKEUP
  - >> SPI_Flash_PowerDown
  - >> SPI_Flash_Erase_Chip
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_Page
  - >> SPI_Flash_Read
  - >> SPI_FLASH_Write_Disable
  - >> SPI_FLASH_Write_Enable
  - >> SPI_FLASH_Write_SR
  - >> SPI_Flash_ReadSR
  - >> SPI_Flash_ReadID
  - >> SPI1_Init

  SPI1_Init (Thumb, 108 bytes, Stack size 8 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SPI1_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> SPI1_ReadWriteByte
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> SD_SPI_Init
  - >> SPI_Flash_Init

  SPI1_SetSpeed (Thumb, 34 bytes, Stack size 0 bytes, spi.o(.text))
  [Called By]

  - >> SD_SPI_SpeedHigh
  - >> SD_SPI_SpeedLow
  - >> SPI_Flash_Init

  SPI_USART_IO_SET (Thumb, 82 bytes, Stack size 0 bytes, flash.o(.text))
  [Called By]

  - >> SPI_Flash_Write
  - >> SPI_Flash_Read

  SPI_Flash_ReadID (Thumb, 66 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_Flash_ReadID ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Init

  SPI_Flash_Init (Thumb, 64 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SPI_Flash_Init ⇒ SPI1_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Flash_ReadID
  - >> SPI1_SetSpeed
  - >> SPI1_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> disk_initialize

  SPI_Flash_ReadSR (Thumb, 38 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Wait_Busy

  SPI_FLASH_Write_SR (Thumb, 34 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte

  SPI_FLASH_Write_Enable (Thumb, 26 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_FLASH_Write_Enable ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Erase_Chip
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_Page

  SPI_FLASH_Write_Disable (Thumb, 26 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte

  SPI_Flash_Read (Thumb, 86 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SPI_Flash_Read ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI_USART_IO_SET
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Write
  - >> Get_HzMat
  - >> ff_convert
  - >> disk_read

  SPI_Flash_Wait_Busy (Thumb, 16 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI_Flash_ReadSR
  [Called By]
  - >> SPI_Flash_Erase_Chip
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_Page

  SPI_Flash_Write_Page (Thumb, 82 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Wait_Busy
  - >> SPI_FLASH_Write_Enable
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Write_NoCheck

  SPI_Flash_Write_NoCheck (Thumb, 70 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Write_Page
  [Called By]
  - >> SPI_Flash_Write

  SPI_Flash_Erase_Sector (Thumb, 64 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SPI_Flash_Erase_Sector ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Wait_Busy
  - >> SPI_FLASH_Write_Enable
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Write

  SPI_Flash_Write (Thumb, 208 bytes, Stack size 40 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> mymalloc
  - >> myfree
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_NoCheck
  - >> SPI_Flash_Read
  - >> SPI_USART_IO_SET
  [Called By]
  - >> disk_write

  SPI_Flash_Erase_Chip (Thumb, 38 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI_Flash_Wait_Busy
  - >> SPI_FLASH_Write_Enable
  - >> SPI1_ReadWriteByte

  SPI_Flash_PowerDown (Thumb, 32 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> delay_us

  SPI_Flash_WAKEUP (Thumb, 32 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> delay_us

  SD_SPI_ReadWriteByte (Thumb, 12 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SD_Initialize
  - >> SD_SendCmd
  - >> SD_SendBlock
  - >> SD_RecvData
  - >> SD_GetResponse
  - >> SD_WaitReady
  - >> SD_DisSelect
  - >> disk_read
  - >> disk_initialize

  SD_SPI_SpeedLow (Thumb, 10 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SD_SPI_SpeedLow
  [Calls]
  - >> SPI1_SetSpeed
  [Called By]
  - >> SD_Initialize
  - >> disk_read
  - >> disk_initialize

  SD_SPI_SpeedHigh (Thumb, 10 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SD_SPI_SpeedHigh
  [Calls]
  - >> SPI1_SetSpeed
  [Called By]
  - >> SD_Initialize
  - >> disk_read
  - >> disk_initialize

  SD_SPI_Init (Thumb, 56 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_SPI_Init ⇒ SPI1_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI1_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> SD_Initialize

  SD_DisSelect (Thumb, 18 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_DisSelect ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_WriteDisk
  - >> SD_ReadDisk
  - >> SD_Initialize
  - >> SD_GetCSD
  - >> SD_GetCID
  - >> SD_SendCmd
  - >> SD_Select

  SD_WaitReady (Thumb, 34 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_SendBlock
  - >> SD_Select
  - >> disk_ioctl

  SD_Select (Thumb, 26 bytes, Stack size 8 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_WaitReady
  - >> SD_DisSelect
  [Called By]
  - >> SD_SendCmd

  SD_GetResponse (Thumb, 38 bytes, Stack size 16 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_GetResponse ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_RecvData

  SD_RecvData (Thumb, 56 bytes, Stack size 16 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SD_RecvData ⇒ SD_GetResponse ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_GetResponse
  - >> SD_SPI_ReadWriteByte
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SD_ReadDisk
  - >> SD_GetCSD
  - >> SD_GetCID

  SD_SendBlock (Thumb, 82 bytes, Stack size 16 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = SD_SendBlock ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_WaitReady
  - >> SD_SPI_ReadWriteByte
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> SD_WriteDisk

  SD_SendCmd (Thumb, 120 bytes, Stack size 24 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_Select
  - >> SD_DisSelect
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> SD_WriteDisk
  - >> SD_ReadDisk
  - >> SD_Initialize
  - >> SD_GetCSD
  - >> SD_GetCID

  SD_GetCID (Thumb, 42 bytes, Stack size 16 bytes, mmc_sd.o(.text), UNUSED)
  [Calls]

  - >> SD_SendCmd
  - >> SD_RecvData
  - >> SD_DisSelect

  SD_GetCSD (Thumb, 42 bytes, Stack size 16 bytes, mmc_sd.o(.text), UNUSED)
  [Calls]

  - >> SD_SendCmd
  - >> SD_RecvData
  - >> SD_DisSelect
  [Called By]
  - >> SD_GetSectorCount

  SD_GetSectorCount (Thumb, 118 bytes, Stack size 32 bytes, mmc_sd.o(.text), UNUSED)
  [Calls]

  - >> SD_GetCSD
  [Called By]
  - >> disk_ioctl

  SD_Initialize (Thumb, 400 bytes, Stack size 24 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = SD_Initialize ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_SendCmd
  - >> SD_DisSelect
  - >> SD_SPI_Init
  - >> SD_SPI_SpeedHigh
  - >> SD_SPI_SpeedLow
  - >> SD_SPI_ReadWriteByte
  [Called By]
  - >> disk_initialize

  SD_ReadDisk (Thumb, 112 bytes, Stack size 24 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = SD_ReadDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_SendCmd
  - >> SD_RecvData
  - >> SD_DisSelect
  [Called By]
  - >> disk_read

  SD_WriteDisk (Thumb, 140 bytes, Stack size 24 bytes, mmc_sd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = SD_WriteDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_SendCmd
  - >> SD_SendBlock
  - >> SD_DisSelect
  [Called By]
  - >> disk_write

  IIC_Init (Thumb, 52 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> AT24CXX_Init

  IIC_Start (Thumb, 68 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Start
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Stop (Thumb, 66 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Stop
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte
  - >> IIC_Wait_Ack

  IIC_Wait_Ack (Thumb, 82 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Wait_Ack ⇒ IIC_Stop
  [Calls]
  - >> IIC_Stop
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Ack (Thumb, 72 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Ack
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_NAck (Thumb, 72 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_NAck
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_Send_Byte (Thumb, 96 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Send_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Read_Byte (Thumb, 98 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_NAck
  - >> IIC_Ack
  - >> delay_us
  [Called By]
  - >> AT24CXX_ReadOneByte

  AT24CXX_Init (Thumb, 8 bytes, Stack size 8 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = AT24CXX_Init ⇒ IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Init
  [Called By]
  - >> TP_Init

  AT24CXX_ReadOneByte (Thumb, 88 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  [Called By]
  - >> TP_Get_Adjdata
  - >> AT24CXX_Read
  - >> AT24CXX_Check
  - >> AT24CXX_ReadLenByte

  AT24CXX_WriteOneByte (Thumb, 80 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> delay_ms
  [Called By]
  - >> TP_Save_Adjdata
  - >> AT24CXX_Write
  - >> AT24CXX_Check
  - >> AT24CXX_WriteLenByte

  AT24CXX_WriteLenByte (Thumb, 42 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Save_Adjdata

  AT24CXX_ReadLenByte (Thumb, 44 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Get_Adjdata

  AT24CXX_Check (Thumb, 46 bytes, Stack size 8 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  AT24CXX_Read (Thumb, 34 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_ReadOneByte

  AT24CXX_Write (Thumb, 36 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte

  TP_Write_Byte (Thumb, 64 bytes, Stack size 0 bytes, touch.o(.text))
  [Called By]

  - >> TP_Read_AD

  TP_Read_AD (Thumb, 124 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TP_Read_AD
  [Calls]
  - >> TP_Write_Byte
  - >> delay_us
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 120 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 38 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Init
  - >> TP_Read_XY2

  TP_Read_XY2 (Thumb, 192 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Drow_Touch_Point (Thumb, 108 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = TP_Drow_Touch_Point ⇒ LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_Draw_Circle
  - >> LCD_DrawLine
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Adjust

  TP_Draw_Big_Point (Thumb, 54 bytes, Stack size 16 bytes, touch.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawPoint

  TP_Scan (Thumb, 262 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY2
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fadd
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Save_Adjdata (Thumb, 130 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = TP_Save_Adjdata ⇒ AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteLenByte
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Get_Adjdata (Thumb, 120 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = TP_Get_Adjdata ⇒ AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadLenByte
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Adj_Info_Show (Thumb, 376 bytes, Stack size 48 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 184
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_ShowNum
  - >> LCD_ShowString
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 1244 bytes, Stack size 80 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> TP_Adj_Info_Show
  - >> TP_Get_Adjdata
  - >> TP_Save_Adjdata
  - >> TP_Drow_Touch_Point
  - >> LCD_Clear
  - >> delay_ms
  - >> LCD_ShowString
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_f2iz
  - >> __aeabi_fdiv
  - >> __aeabi_fsub
  - >> __aeabi_f2d
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> sqrt
  [Called By]
  - >> TP_Init
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Init (Thumb, 170 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 272 + Unknown Stack Size
  - Call Chain = TP_Init ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> OTT2001A_Init
  - >> TP_Adjust
  - >> TP_Get_Adjdata
  - >> TP_Save_Adjdata
  - >> TP_Read_XY
  - >> AT24CXX_Init
  - >> LCD_Clear
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Address Reference Count : 1]
  - touch.o(.data)

  CT_Delay (Thumb, 10 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CT_Delay
  [Calls]
  - >> delay_us
  [Called By]
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_NAck
  - >> CT_IIC_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start

  CT_IIC_Init (Thumb, 46 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CT_IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> OTT2001A_Init

  CT_IIC_Start (Thumb, 60 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Start ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> OTT2001A_RD_Reg
  - >> OTT2001A_WR_Reg

  CT_IIC_Stop (Thumb, 60 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Stop ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> OTT2001A_RD_Reg
  - >> OTT2001A_WR_Reg
  - >> CT_IIC_Wait_Ack

  CT_IIC_Wait_Ack (Thumb, 82 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CT_IIC_Wait_Ack ⇒ CT_IIC_Stop ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_Stop
  - >> delay_us
  [Called By]
  - >> OTT2001A_RD_Reg
  - >> OTT2001A_WR_Reg

  CT_IIC_Ack (Thumb, 64 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Ack ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> CT_IIC_Read_Byte

  CT_IIC_NAck (Thumb, 64 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> CT_IIC_Read_Byte

  CT_IIC_Send_Byte (Thumb, 84 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CT_IIC_Send_Byte ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> OTT2001A_RD_Reg
  - >> OTT2001A_WR_Reg

  CT_IIC_Read_Byte (Thumb, 92 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CT_IIC_Read_Byte ⇒ CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_NAck
  - >> CT_IIC_Ack
  - >> delay_us
  [Called By]
  - >> OTT2001A_RD_Reg

  OTT2001A_WR_Reg (Thumb, 92 bytes, Stack size 24 bytes, ott2001a.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = OTT2001A_WR_Reg ⇒ CT_IIC_Send_Byte ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  [Called By]
  - >> OTT2001A_SensorControl

  OTT2001A_RD_Reg (Thumb, 98 bytes, Stack size 24 bytes, ott2001a.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = OTT2001A_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_Read_Byte
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  [Called By]
  - >> OTT2001A_Init
  - >> CTP_Scan

  OTT2001A_SensorControl (Thumb, 28 bytes, Stack size 16 bytes, ott2001a.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = OTT2001A_SensorControl ⇒ OTT2001A_WR_Reg ⇒ CT_IIC_Send_Byte ⇒ CT_Delay
  [Calls]
  - >> OTT2001A_WR_Reg
  [Called By]
  - >> OTT2001A_Init

  OTT2001A_Init (Thumb, 158 bytes, Stack size 8 bytes, ott2001a.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = OTT2001A_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> OTT2001A_SensorControl
  - >> OTT2001A_RD_Reg
  - >> CT_IIC_Init
  - >> delay_ms
  - >> __2printf
  [Called By]
  - >> TP_Init

  CTP_Scan (Thumb, 440 bytes, Stack size 48 bytes, ott2001a.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = CTP_Scan ⇒ OTT2001A_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> OTT2001A_RD_Reg
  - >> __aeabi_dmul
  - >> __aeabi_i2d
  - >> __aeabi_d2uiz
  - >> __aeabi_drsub
  [Address Reference Count : 1]
  - touch.o(.text)

  TIM4_Set (Thumb, 34 bytes, Stack size 8 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM4_Set
  [Calls]
  - >> TIM_SetCounter
  - >> TIM_Cmd
  [Called By]
  - >> TIM4_IRQHandler
  - >> USART2_IRQHandler
  - >> USART2_Init

  USART2_IRQHandler (Thumb, 84 bytes, Stack size 8 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART2_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> TIM_SetCounter
  - >> TIM4_Set
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM4_Init (Thumb, 82 bytes, Stack size 32 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM4_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> USART2_Init

  UART_DMA_Config (Thumb, 72 bytes, Stack size 64 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> RCC_AHBPeriphClockCmd
  - >> DMA_Init
  - >> DMA_DeInit
  [Called By]
  - >> USART2_Init

  USART2_Init (Thumb, 204 bytes, Stack size 32 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = USART2_Init ⇒ UART_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_DeInit
  - >> USART_DMACmd
  - >> USART_Cmd
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> UART_DMA_Config
  - >> TIM4_Init
  - >> TIM4_Set
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  UART_DMA_Enable (Thumb, 32 bytes, Stack size 16 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMA_Enable
  [Calls]
  - >> DMA_SetCurrDataCounter
  - >> DMA_Cmd
  [Called By]
  - >> u2_printf

  u2_printf (Thumb, 54 bytes, Stack size 32 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = u2_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> UART_DMA_Enable
  - >> strlen
  - >> __c89vsprintf
  [Called By]
  - >> main
  - >> sim900a_gprs_test
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> sim900a_send_cmd

  TIM4_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, usart2.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM4_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  - >> TIM4_Set
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM2_Set (Thumb, 38 bytes, Stack size 8 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM2_Set
  [Calls]
  - >> TIM_SetCounter
  - >> TIM_Cmd
  [Called By]
  - >> TIM2_IRQHandler
  - >> USART3_Init
  - >> USART3_IRQHandler

  USART3_IRQHandler (Thumb, 84 bytes, Stack size 8 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART3_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> TIM2_Set
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> TIM_SetCounter
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM2_Init (Thumb, 84 bytes, Stack size 32 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM2_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> USART3_Init

  UART3_DMA_Config (Thumb, 72 bytes, Stack size 64 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART3_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> RCC_AHBPeriphClockCmd
  - >> DMA_Init
  - >> DMA_DeInit
  [Called By]
  - >> USART3_Init

  USART3_Init (Thumb, 208 bytes, Stack size 32 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = USART3_Init ⇒ UART3_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> UART3_DMA_Config
  - >> TIM2_Init
  - >> TIM2_Set
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_DeInit
  - >> USART_DMACmd
  - >> USART_Cmd
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> HC05_Init

  UART3_DMA_Enable (Thumb, 32 bytes, Stack size 16 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART3_DMA_Enable
  [Calls]
  - >> DMA_SetCurrDataCounter
  - >> DMA_Cmd
  [Called By]
  - >> u3_printf

  u3_printf (Thumb, 56 bytes, Stack size 32 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = u3_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> DMA_GetCurrDataCounter
  - >> UART3_DMA_Enable
  - >> strlen
  - >> __c89vsprintf
  [Called By]
  - >> HC05_Set_Cmd
  - >> HC05_Init
  - >> HC05_Get_Role
  - >> HC05_CFG_CMD

  TIM2_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, usart3.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM2_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM2_Set
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  delay_init (Thumb, 50 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 70 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> CT_IIC_Read_Byte
  - >> CT_IIC_Wait_Ack
  - >> CT_Delay
  - >> TP_Read_AD
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> SPI_Flash_WAKEUP
  - >> SPI_Flash_PowerDown
  - >> LCD_ReadPoint
  - >> LCD_RD_DATA
  - >> LCD_Init

  delay_ms (Thumb, 70 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> OTT2001A_Init
  - >> TP_Adjust
  - >> AT24CXX_WriteOneByte
  - >> sim900a_test
  - >> LCD_Init
  - >> KEY_Scan
  - >> HC05_Set_Cmd
  - >> HC05_Init
  - >> HC05_Get_Role
  - >> main
  - >> HC05_CFG_CMD
  - >> sim900a_gprs_test
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> sim900a_send_cmd

  NVIC_Configuration (Thumb, 12 bytes, Stack size 8 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_Configuration
  [Calls]
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 22 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - _printf_char_file.o(.text)

  uart_init (Thumb, 158 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_DeInit
  - >> USART_Cmd
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 122 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 274 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> USART3_Init
  - >> CT_IIC_Init
  - >> TP_Init
  - >> IIC_Init
  - >> SD_SPI_Init
  - >> SPI_Flash_Init
  - >> SPI1_Init
  - >> uart_init
  - >> USART2_Init
  - >> LED_Init
  - >> LCD_Init
  - >> KEY_Init
  - >> HC05_Init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> KEY_Scan

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> LCD_ReadPoint
  - >> LCD_RD_DATA

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> CT_IIC_Init
  - >> SD_SPI_Init
  - >> SPI_Flash_Init
  - >> SPI1_Init
  - >> LCD_Color_Fill
  - >> LCD_Clear
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_ReadPoint
  - >> LCD_SetCursor
  - >> LCD_WriteRAM
  - >> LCD_WriteReg
  - >> LCD_RD_DATA
  - >> LCD_WR_DATAX
  - >> LCD_WR_REG
  - >> LED_Init
  - >> LCD_Init
  - >> LCD_Fill
  - >> HC05_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> LCD_Color_Fill
  - >> LCD_Clear
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_ReadPoint
  - >> LCD_SetCursor
  - >> LCD_WriteRAM
  - >> LCD_WriteReg
  - >> LCD_RD_DATA
  - >> LCD_WR_DATAX
  - >> LCD_WR_REG
  - >> LCD_Fill

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> LCD_Color_Fill
  - >> LCD_Clear
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_SetCursor
  - >> LCD_WriteRAM
  - >> LCD_WriteReg
  - >> LCD_WR_DATAX
  - >> LCD_WR_REG
  - >> LCD_Fill

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> LCD_Init
  - >> KEY_Init

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 44 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> I2S_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> UART3_DMA_Config
  - >> UART_DMA_Config

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> USART3_Init
  - >> CT_IIC_Init
  - >> TP_Init
  - >> IIC_Init
  - >> SD_SPI_Init
  - >> SPI_Flash_Init
  - >> SPI1_Init
  - >> uart_init
  - >> USART2_Init
  - >> LED_Init
  - >> LCD_Init
  - >> KEY_Init
  - >> HC05_Init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> USART3_Init
  - >> TIM2_Init
  - >> TIM4_Init
  - >> USART2_Init

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit
  - >> USART_DeInit
  - >> TIM_DeInit
  - >> SPI_I2S_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> USART_DeInit
  - >> TIM_DeInit
  - >> SPI_I2S_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> USART3_Init
  - >> uart_init
  - >> USART2_Init

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART3_Init
  - >> uart_init
  - >> USART2_Init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART3_Init
  - >> uart_init
  - >> USART2_Init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> USART3_Init
  - >> uart_init
  - >> USART2_Init

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART3_Init
  - >> USART2_Init

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler
  - >> USART3_IRQHandler
  - >> USART2_IRQHandler

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler
  - >> USART3_IRQHandler
  - >> USART2_IRQHandler

  USART_ClearITPendingBit (Thumb, 52 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 102 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> USART3_Init
  - >> TIM2_Init
  - >> TIM4_Init
  - >> uart_init
  - >> USART2_Init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI1_Init

  I2S_Init (Thumb, 226 bytes, Stack size 56 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_Init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 32 bytes, Stack size 12 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)

  TIM_DeInit (Thumb, 424 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 122 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM2_Init
  - >> TIM4_Init

  TIM_OC1Init (Thumb, 132 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 154 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 150 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 182 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 150 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config

  TIM_PWMIConfig (Thumb, 124 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_BDTRConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 40 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM2_Set
  - >> TIM4_Set

  TIM_CtrlPWMOutputs (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM2_Init
  - >> TIM4_Init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMAConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 62 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 28 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 54 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 32 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 66 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 82 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> USART3_IRQHandler
  - >> TIM2_Set
  - >> USART2_IRQHandler
  - >> TIM4_Set

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture1 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetPrescaler (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM2_IRQHandler
  - >> TIM4_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM2_IRQHandler
  - >> TIM4_IRQHandler

  DMA_DeInit (Thumb, 324 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> UART3_DMA_Config
  - >> UART_DMA_Config

  DMA_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_dma.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_Init
  [Called By]
  - >> UART3_DMA_Config
  - >> UART_DMA_Config

  DMA_StructInit (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> UART3_DMA_Enable
  - >> UART_DMA_Enable

  DMA_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> UART3_DMA_Enable
  - >> UART_DMA_Enable

  DMA_GetCurrDataCounter (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> u3_printf

  DMA_GetFlagStatus (Thumb, 38 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_ClearFlag (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_GetITStatus (Thumb, 38 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_ClearITPendingBit (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  mymemcpy (Thumb, 26 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Called By]

  - >> myrealloc

  mymemset (Thumb, 20 bytes, Stack size 12 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = mymemset
  [Called By]
  - >> mem_init

  mem_init (Thumb, 38 bytes, Stack size 4 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = mem_init ⇒ mymemset
  [Calls]
  - >> mymemset
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - malloc.o(.data)

  mem_perused (Thumb, 42 bytes, Stack size 0 bytes, malloc.o(.text))
  [Address Reference Count : 1]

  - malloc.o(.data)

  mem_malloc (Thumb, 116 bytes, Stack size 24 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = mem_malloc
  [Called By]
  - >> mymalloc
  - >> myrealloc

  mem_free (Thumb, 66 bytes, Stack size 16 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = mem_free
  [Called By]
  - >> myfree

  myfree (Thumb, 24 bytes, Stack size 16 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = myfree ⇒ mem_free
  [Calls]
  - >> mem_free
  [Called By]
  - >> SPI_Flash_Write
  - >> sim900a_gsminfo_show
  - >> sim900a_mtest_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> ff_memfree
  - >> myrealloc

  mymalloc (Thumb, 26 bytes, Stack size 16 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = mymalloc ⇒ mem_malloc
  [Calls]
  - >> mem_malloc
  [Called By]
  - >> SPI_Flash_Write
  - >> exfuns_init
  - >> sim900a_gsminfo_show
  - >> sim900a_mtest_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> ff_memalloc

  myrealloc (Thumb, 48 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Calls]

  - >> myfree
  - >> mem_malloc
  - >> mymemcpy

  exfuns_init (Thumb, 100 bytes, Stack size 8 bytes, exfuns.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = exfuns_init ⇒ mymalloc ⇒ mem_malloc
  [Calls]
  - >> mymalloc
  [Called By]
  - >> main

  char_upper (Thumb, 26 bytes, Stack size 0 bytes, exfuns.o(.text), UNUSED)
  [Called By]

  - >> f_typetell

  f_typetell (Thumb, 188 bytes, Stack size 32 bytes, exfuns.o(.text), UNUSED)
  [Calls]

  - >> strcmp
  - >> strcpy
  - >> char_upper

  exf_getfree (Thumb, 74 bytes, Stack size 40 bytes, exfuns.o(.text), UNUSED)
  [Calls]

  - >> f_getfree

  disk_initialize (Thumb, 88 bytes, Stack size 16 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = disk_initialize ⇒ SD_Initialize ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_Initialize
  - >> SD_SPI_SpeedHigh
  - >> SD_SPI_SpeedLow
  - >> SD_SPI_ReadWriteByte
  - >> SPI_Flash_Init
  [Called By]
  - >> find_volume
  - >> f_mkfs

  disk_status (Thumb, 6 bytes, Stack size 0 bytes, diskio.o(.text))
  [Called By]

  - >> validate
  - >> find_volume

  disk_read (Thumb, 118 bytes, Stack size 24 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = disk_read ⇒ SD_ReadDisk ⇒ SD_SendCmd ⇒ SD_Select ⇒ SD_WaitReady ⇒ SD_SPI_ReadWriteByte ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_ReadDisk
  - >> SD_SPI_SpeedHigh
  - >> SD_SPI_SpeedLow
  - >> SD_SPI_ReadWriteByte
  - >> SPI_Flash_Read
  [Called By]
  - >> move_window
  - >> f_write
  - >> f_read
  - >> f_lseek

  disk_write (Thumb, 98 bytes, Stack size 24 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SD_WriteDisk
  - >> SPI_Flash_Write
  [Called By]
  - >> f_truncate
  - >> f_sync
  - >> sync_fs
  - >> sync_window
  - >> f_write
  - >> f_read
  - >> f_mkfs
  - >> f_lseek

  disk_ioctl (Thumb, 154 bytes, Stack size 24 bytes, diskio.o(.text), UNUSED)
  [Calls]

  - >> SD_GetSectorCount
  - >> SD_WaitReady
  [Called By]
  - >> sync_fs
  - >> f_mkfs

  get_fattime (Thumb, 4 bytes, Stack size 0 bytes, diskio.o(.text), UNUSED)
  [Called By]

  - >> f_sync
  - >> f_setlabel
  - >> f_open
  - >> f_mkfs
  - >> f_mkdir

  ff_memalloc (Thumb, 12 bytes, Stack size 8 bytes, diskio.o(.text), UNUSED)
  [Calls]

  - >> mymalloc
  [Called By]
  - >> f_utime
  - >> f_chmod
  - >> f_stat
  - >> f_unlink
  - >> f_rename
  - >> f_readdir
  - >> f_opendir
  - >> f_open
  - >> f_mkdir

  ff_memfree (Thumb, 12 bytes, Stack size 8 bytes, diskio.o(.text), UNUSED)
  [Calls]

  - >> myfree
  [Called By]
  - >> f_utime
  - >> f_chmod
  - >> f_stat
  - >> f_unlink
  - >> f_rename
  - >> f_readdir
  - >> f_opendir
  - >> f_open
  - >> f_mkdir

  clust2sect (Thumb, 26 bytes, Stack size 0 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> dir_next
  - >> dir_sdi
  - >> f_write
  - >> f_rename
  - >> f_read
  - >> f_mkdir
  - >> f_lseek

  get_fat (Thumb, 232 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> move_window
  [Called By]
  - >> f_truncate
  - >> dir_next
  - >> dir_sdi
  - >> create_chain
  - >> remove_chain
  - >> f_read
  - >> f_lseek
  - >> f_getfree

  put_fat (Thumb, 316 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> move_window
  [Called By]
  - >> f_truncate
  - >> create_chain
  - >> remove_chain

  f_mount (Thumb, 86 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 312
  - Call Chain = f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> find_volume
  - >> get_ldnumber
  [Called By]
  - >> main

  f_open (Thumb, 380 bytes, Stack size 96 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> dir_register
  - >> st_clust
  - >> ld_clust
  - >> remove_chain
  - >> move_window
  - >> ff_memfree
  - >> ff_memalloc
  - >> get_fattime

  f_read (Thumb, 446 bytes, Stack size 64 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> clust2sect
  - >> validate
  - >> clmt_clust
  - >> mem_cpy
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> f_gets

  f_write (Thumb, 496 bytes, Stack size 64 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect
  - >> validate
  - >> clmt_clust
  - >> create_chain
  - >> mem_cpy
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> f_printf
  - >> putc_bfd
  - >> f_puts
  - >> f_putc

  f_sync (Thumb, 174 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> validate
  - >> st_clust
  - >> sync_fs
  - >> move_window
  - >> get_fattime
  - >> disk_write
  [Called By]
  - >> f_close

  f_close (Thumb, 32 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_sync
  - >> validate

  f_lseek (Thumb, 652 bytes, Stack size 48 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> clust2sect
  - >> validate
  - >> clmt_clust
  - >> create_chain
  - >> disk_write
  - >> disk_read

  f_opendir (Thumb, 136 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> ld_clust
  - >> dir_sdi
  - >> ff_memfree
  - >> ff_memalloc

  f_closedir (Thumb, 22 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> validate

  f_readdir (Thumb, 114 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> validate
  - >> get_fileinfo
  - >> dir_read
  - >> dir_next
  - >> dir_sdi
  - >> ff_memfree
  - >> ff_memalloc

  f_stat (Thumb, 84 bytes, Stack size 72 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> get_fileinfo
  - >> ff_memfree
  - >> ff_memalloc

  f_getfree (Thumb, 258 bytes, Stack size 56 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> find_volume
  - >> move_window
  [Called By]
  - >> exf_getfree

  f_truncate (Thumb, 184 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> put_fat
  - >> get_fat
  - >> validate
  - >> remove_chain
  - >> disk_write

  f_unlink (Thumb, 194 bytes, Stack size 112 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> dir_remove
  - >> dir_read
  - >> ld_clust
  - >> dir_sdi
  - >> remove_chain
  - >> sync_fs
  - >> mem_cpy
  - >> ff_memfree
  - >> ff_memalloc

  f_mkdir (Thumb, 380 bytes, Stack size 88 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect
  - >> find_volume
  - >> follow_path
  - >> dir_register
  - >> st_clust
  - >> create_chain
  - >> remove_chain
  - >> sync_fs
  - >> sync_window
  - >> mem_set
  - >> mem_cpy
  - >> ff_memfree
  - >> ff_memalloc
  - >> get_fattime

  f_chmod (Thumb, 112 bytes, Stack size 88 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> sync_fs
  - >> ff_memfree
  - >> ff_memalloc

  f_utime (Thumb, 110 bytes, Stack size 80 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> sync_fs
  - >> ff_memfree
  - >> ff_memalloc

  f_rename (Thumb, 314 bytes, Stack size 144 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect
  - >> find_volume
  - >> get_ldnumber
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> st_clust
  - >> ld_clust
  - >> sync_fs
  - >> move_window
  - >> mem_cpy
  - >> ff_memfree
  - >> ff_memalloc

  f_getlabel (Thumb, 190 bytes, Stack size 72 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> dir_read
  - >> dir_sdi
  - >> move_window
  - >> mem_cpy

  f_setlabel (Thumb, 468 bytes, Stack size 88 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> ff_wtoupper
  - >> ff_convert
  - >> find_volume
  - >> dir_read
  - >> dir_alloc
  - >> dir_sdi
  - >> sync_fs
  - >> chk_chr
  - >> mem_set
  - >> mem_cpy
  - >> get_fattime

  f_mkfs (Thumb, 1570 bytes, Stack size 112 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_ldnumber
  - >> mem_set
  - >> mem_cpy
  - >> get_fattime
  - >> disk_ioctl
  - >> disk_write
  - >> disk_initialize

  f_gets (Thumb, 82 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_read

  f_putc (Thumb, 64 bytes, Stack size 96 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> putc_bfd
  - >> f_write

  f_puts (Thumb, 74 bytes, Stack size 96 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> putc_bfd
  - >> f_write

  f_printf (Thumb, 674 bytes, Stack size 160 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> putc_bfd
  - >> f_write

  ff_convert (Thumb, 146 bytes, Stack size 40 bytes, mycc936.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = ff_convert ⇒ SPI_Flash_Read ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Read
  [Called By]
  - >> sim900a_unigbk_exchange
  - >> create_name
  - >> get_fileinfo
  - >> f_setlabel

  ff_wtoupper (Thumb, 46 bytes, Stack size 0 bytes, mycc936.o(.text), UNUSED)
  [Called By]

  - >> create_name
  - >> cmp_lfn
  - >> f_setlabel

  Get_HzMat (Thumb, 220 bytes, Stack size 40 bytes, text.o(.text), UNUSED)
  [Calls]

  - >> SPI_Flash_Read
  [Called By]
  - >> Show_Font

  Show_Font (Thumb, 190 bytes, Stack size 128 bytes, text.o(.text), UNUSED)
  [Calls]

  - >> LCD_Fast_DrawPoint
  - >> Get_HzMat
  [Called By]
  - >> Show_Str

  Show_Str (Thumb, 192 bytes, Stack size 48 bytes, text.o(.text), UNUSED)
  [Calls]

  - >> LCD_ShowChar
  - >> Show_Font
  [Called By]
  - >> sim900a_mtest_ui
  - >> sim900a_gprs_test
  - >> sim900a_gprs_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> Show_Str_Mid

  Show_Str_Mid (Thumb, 106 bytes, Stack size 40 bytes, text.o(.text), UNUSED)
  [Calls]

  - >> strlen
  - >> Show_Str
  [Called By]
  - >> sim900a_mtest_ui
  - >> sim900a_gprs_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> sim900a_key_staset
  - >> sim900a_load_keyboard

  sim_at_response (Thumb, 46 bytes, Stack size 8 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = sim_at_response ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> sim900a_test
  - >> sim900a_gprs_test
  - >> sim900a_sms_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test

  sim900a_check_cmd (Thumb, 44 bytes, Stack size 16 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = sim900a_check_cmd ⇒ strstr
  [Calls]
  - >> strstr
  [Called By]
  - >> sim900a_call_test
  - >> sim900a_send_cmd

  sim900a_send_cmd (Thumb, 104 bytes, Stack size 24 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = sim900a_send_cmd ⇒ u2_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> u2_printf
  - >> delay_ms
  - >> sim900a_check_cmd
  [Called By]
  - >> sim900a_test
  - >> sim900a_gsminfo_show
  - >> sim900a_mtest_ui
  - >> sim900a_gprs_test
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test

  sim900a_chr2hex (Thumb, 54 bytes, Stack size 0 bytes, sim900a.o(.text))
  [Called By]

  - >> sim900a_unigbk_exchange

  sim900a_hex2chr (Thumb, 34 bytes, Stack size 0 bytes, sim900a.o(.text))
  [Called By]

  - >> sim900a_unigbk_exchange

  sim900a_unigbk_exchange (Thumb, 236 bytes, Stack size 24 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = sim900a_unigbk_exchange ⇒ ff_convert ⇒ SPI_Flash_Read ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> sim900a_hex2chr
  - >> sim900a_chr2hex
  - >> ff_convert
  [Called By]
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test

  sim900a_load_keyboard (Thumb, 292 bytes, Stack size 32 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawRectangle
  - >> LCD_Fill
  - >> Show_Str_Mid
  [Called By]
  - >> sim900a_gprs_ui
  - >> sim900a_sms_read_test
  - >> sim900a_call_test

  sim900a_key_staset (Thumb, 338 bytes, Stack size 32 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> LCD_Fill
  - >> Show_Str_Mid
  [Called By]
  - >> sim900a_get_keynum

  sim900a_get_keynum (Thumb, 228 bytes, Stack size 24 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> sim900a_key_staset
  [Called By]
  - >> sim900a_gprs_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test

  sim900a_call_test (Thumb, 1190 bytes, Stack size 72 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> mymalloc
  - >> myfree
  - >> LCD_ShowChar
  - >> LCD_Clear
  - >> u2_printf
  - >> delay_ms
  - >> LCD_Fill
  - >> strcpy
  - >> strstr
  - >> sim900a_get_keynum
  - >> sim900a_load_keyboard
  - >> sim900a_send_cmd
  - >> sim900a_check_cmd
  - >> sim_at_response
  - >> Show_Str_Mid
  - >> Show_Str

  sim900a_sms_read_test (Thumb, 1242 bytes, Stack size 56 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> mymalloc
  - >> myfree
  - >> LCD_Clear
  - >> u2_printf
  - >> delay_ms
  - >> LCD_Fill
  - >> strstr
  - >> __2sprintf
  - >> sim900a_get_keynum
  - >> sim900a_load_keyboard
  - >> sim900a_unigbk_exchange
  - >> sim900a_send_cmd
  - >> sim_at_response
  - >> Show_Str_Mid
  - >> Show_Str

  sim900a_sms_send_test (Thumb, 226 bytes, Stack size 48 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = sim900a_sms_send_test ⇒ sim900a_send_cmd ⇒ u2_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> mymalloc
  - >> myfree
  - >> u2_printf
  - >> delay_ms
  - >> __aeabi_memcpy4
  - >> __2sprintf
  - >> sim900a_unigbk_exchange
  - >> sim900a_send_cmd
  - >> sim_at_response
  [Called By]
  - >> sim900a_sms_test

  sim900a_sms_ui (Thumb, 24 bytes, Stack size 16 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> LCD_Clear

  sim900a_sms_test (Thumb, 88 bytes, Stack size 8 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = sim900a_sms_test ⇒ sim900a_sms_send_test ⇒ sim900a_send_cmd ⇒ u2_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> sim900a_sms_send_test
  - >> sim900a_send_cmd
  - >> sim_at_response
  [Called By]
  - >> sim900a_test

  sim900a_tcpudp_test (Thumb, 1498 bytes, Stack size 88 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> mymalloc
  - >> myfree
  - >> LCD_Clear
  - >> u2_printf
  - >> delay_ms
  - >> LCD_Fill
  - >> KEY_Scan
  - >> strstr
  - >> __2sprintf
  - >> __2printf
  - >> sim900a_send_cmd
  - >> Show_Str_Mid
  - >> Show_Str
  [Called By]
  - >> sim900a_gprs_test

  sim900a_gprs_ui (Thumb, 154 bytes, Stack size 16 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> LCD_Clear
  - >> sim900a_load_keyboard
  - >> Show_Str_Mid
  - >> Show_Str
  [Called By]
  - >> sim900a_gprs_test

  sim900a_gprs_test (Thumb, 864 bytes, Stack size 56 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> u2_printf
  - >> delay_ms
  - >> LCD_Fill
  - >> KEY_Scan
  - >> sim900a_gprs_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_get_keynum
  - >> sim900a_send_cmd
  - >> sim_at_response
  - >> Show_Str

  sim900a_mtest_ui (Thumb, 476 bytes, Stack size 40 bytes, sim900a.o(.text), UNUSED)
  [Calls]

  - >> mymalloc
  - >> myfree
  - >> LCD_Clear
  - >> strstr
  - >> __2sprintf
  - >> sim900a_send_cmd
  - >> Show_Str_Mid
  - >> Show_Str

  sim900a_gsminfo_show (Thumb, 560 bytes, Stack size 32 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = sim900a_gsminfo_show ⇒ sim900a_send_cmd ⇒ u2_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> mymalloc
  - >> myfree
  - >> strstr
  - >> sim900a_send_cmd
  [Called By]
  - >> sim900a_test

  sim900a_test (Thumb, 104 bytes, Stack size 16 bytes, sim900a.o(.text))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = sim900a_test ⇒ sim900a_sms_test ⇒ sim900a_sms_send_test ⇒ sim900a_send_cmd ⇒ u2_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> sim900a_gsminfo_show
  - >> sim900a_sms_test
  - >> sim900a_send_cmd
  - >> sim_at_response
  [Called By]
  - >> main

  HC05_Init (Thumb, 206 bytes, Stack size 24 bytes, hc05.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = HC05_Init ⇒ u3_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> u3_printf
  - >> USART3_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> delay_ms
  [Called By]
  - >> main

  HC05_Get_Role (Thumb, 126 bytes, Stack size 16 bytes, hc05.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = HC05_Get_Role ⇒ u3_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> u3_printf
  - >> delay_ms
  [Called By]
  - >> main
  - >> HC05_Role_Show

  HC05_Set_Cmd (Thumb, 130 bytes, Stack size 24 bytes, hc05.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = HC05_Set_Cmd ⇒ u3_printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> u3_printf
  - >> delay_ms
  [Called By]
  - >> main

  HC05_CFG_CMD (Thumb, 96 bytes, Stack size 16 bytes, hc05.o(.text), UNUSED)
  [Calls]

  - >> u3_printf
  - >> delay_ms
  - >> __2printf

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __c89vsprintf (Thumb, 32 bytes, Stack size 16 bytes, c89vsprintf.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> u3_printf
  - >> u2_printf

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, __2printf.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> OTT2001A_Init
  - >> LCD_Init
  - >> HC05_CFG_CMD
  - >> sim900a_tcpudp_test
  - >> sim_at_response

  __2sprintf (Thumb, 38 bytes, Stack size 32 bytes, __2sprintf.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> main
  - >> sim900a_mtest_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_send_test
  - >> sim900a_sms_read_test

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 102 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  - >> _printf_truncate_unsigned
  - >> _printf_truncate_signed
  [Called By]
  - >> _printf_d
  - >> _printf_u
  - >> _printf_i

  _printf_longlong_hex (Thumb, 92 bytes, Stack size 16 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_hex_ptr
  - >> _printf_ll_hex
  - >> _printf_int_hex

  _printf_int_hex (Thumb, 28 bytes, Stack size 16 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _printf_int_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  - >> _printf_truncate_unsigned
  [Called By]
  - >> _printf_x

  _printf_ll_hex (Thumb, 12 bytes, Stack size 0 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_ll_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  [Called By]
  - >> _printf_llx

  _printf_hex_ptr (Thumb, 18 bytes, Stack size 0 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_hex_ptr ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  [Called By]
  - >> _printf_p

  __printf (Thumb, 390 bytes, Stack size 40 bytes, __printf_flags_ss_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> sim900a_gsminfo_show
  - >> sim900a_mtest_ui
  - >> sim900a_tcpudp_test
  - >> sim900a_sms_read_test
  - >> sim900a_call_test
  - >> sim900a_check_cmd

  strcpy (Thumb, 72 bytes, Stack size 12 bytes, strcpy.o(.text), UNUSED)
  [Called By]

  - >> sim900a_call_test
  - >> f_typetell

  strlen (Thumb, 62 bytes, Stack size 8 bytes, strlen.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strlen
  [Called By]
  - >> u3_printf
  - >> u2_printf
  - >> Show_Str_Mid

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy4
  [Called By]
  - >> sim900a_sms_send_test

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> f_typetell
  - >> _get_lc_ctype
  - >> _get_lc_numeric

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_errno_addr

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> sqrt

  _printf_pre_padding (Thumb, 46 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_str
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_wctomb
  - >> _printf_int_common

  _printf_post_padding (Thumb, 36 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_str
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_wctomb
  - >> _printf_int_common

  _printf_truncate_signed (Thumb, 18 bytes, Stack size 0 bytes, _printf_truncate.o(.text))
  [Called By]

  - >> _printf_int_dec

  _printf_truncate_unsigned (Thumb, 18 bytes, Stack size 0 bytes, _printf_truncate.o(.text))
  [Called By]

  - >> _printf_int_hex
  - >> _printf_int_dec
  - >> _printf_int_oct

  _printf_int_common (Thumb, 184 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_longlong_hex
  - >> _printf_int_dec
  - >> _printf_longlong_oct
  - >> _printf_longlong_dec

  _printf_charcount (Thumb, 42 bytes, Stack size 0 bytes, _printf_charcount.o(.text))
  [Called By]

  - >> _printf_n

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> __2sprintf
  - >> __c89vsprintf
  - >> _printf_char_file

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __2sprintf
  - >> __c89vsprintf
  [Address Reference Count : 2]
  - c89vsprintf.o(.text)
  - __2sprintf.o(.text)

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_c

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  _printf_wctomb (Thumb, 182 bytes, Stack size 56 bytes, _printf_wctomb.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _wcrtomb
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_lcs_common

  _printf_longlong_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_longlong_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _ll_udiv10
  - >> _printf_int_common
  [Called By]
  - >> _printf_llu
  - >> _printf_lld
  - >> _printf_lli

  _printf_longlong_oct (Thumb, 76 bytes, Stack size 8 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_ll_oct
  - >> _printf_int_oct

  _printf_int_oct (Thumb, 24 bytes, Stack size 8 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_oct
  - >> _printf_truncate_unsigned
  [Called By]
  - >> _printf_o

  _printf_ll_oct (Thumb, 12 bytes, Stack size 0 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_ll_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_oct
  [Called By]
  - >> _printf_llo

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> __set_errno
  - >> __read_errno

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  _ll_udiv10 (Thumb, 138 bytes, Stack size 12 bytes, lludiv10.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = _ll_udiv10
  [Called By]
  - >> _fp_digits
  - >> _printf_longlong_dec

  __lib_sel_fp_printf (Thumb, 2 bytes, Stack size 0 bytes, _printf_fp_dec.o(.text), UNUSED)

  _printf_fp_dec_real (Thumb, 628 bytes, Stack size 104 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 320
  - Call Chain = _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> __ARM_fpclassify
  - >> _printf_fp_infnan
  - >> __rt_locale
  - >> _fp_digits
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec

  _printf_lcs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wctomb
  [Called By]
  - >> _printf_wstring
  - >> _printf_wchar

  _printf_wchar (Thumb, 16 bytes, Stack size 0 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_wchar ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_lcs_common
  [Called By]
  - >> _printf_lc

  _printf_wstring (Thumb, 8 bytes, Stack size 0 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_wstring ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_lcs_common
  [Called By]
  - >> _printf_ls

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  _wcrtomb (Thumb, 64 bytes, Stack size 16 bytes, _wcrtomb.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> __rt_ctype_table
  [Called By]
  - >> _printf_wctomb

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  __rt_ctype_table (Thumb, 16 bytes, Stack size 8 bytes, rt_ctype_table.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __rt_ctype_table
  [Calls]
  - >> __rt_locale
  [Called By]
  - >> _wcrtomb

  __rt_locale (Thumb, 8 bytes, Stack size 0 bytes, rt_locale_intlibspace.o(.text))
  [Called By]

  - >> __rt_lib_init_lc_common
  - >> __rt_ctype_table
  - >> _printf_fp_dec_real

  _printf_fp_infnan (Thumb, 112 bytes, Stack size 24 bytes, _printf_fp_infnan.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_fp_infnan ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec_real

  _btod_etento (Thumb, 222 bytes, Stack size 72 bytes, bigflt0.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  [Called By]
  - >> _fp_digits

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  _btod_d2e (Thumb, 62 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e))
  [Calls]

  - >> _d2e_norm_op1
  [Called By]
  - >> _fp_digits

  _d2e_denorm_low (Thumb, 70 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_denorm_low))
  [Called By]

  - >> _d2e_norm_op1

  _d2e_norm_op1 (Thumb, 96 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_norm_op1))
  [Calls]

  - >> _d2e_denorm_low
  [Called By]
  - >> _btod_d2e

  __btod_div_common (Thumb, 696 bytes, Stack size 24 bytes, btod.o(CL$$btod_div_common))
  [Stack]

  - Max Depth = 24
  - Call Chain = __btod_div_common
  [Called By]
  - >> _btod_ediv

  _e2e (Thumb, 198 bytes, Stack size 24 bytes, btod.o(CL$$btod_e2e))
  [Stack]

  - Max Depth = 24
  - Call Chain = _e2e
  [Called By]
  - >> _btod_emul
  - >> _btod_ediv

  _btod_ediv (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_ediv))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_ediv ⇒ _e2e
  [Calls]
  - >> _e2e
  - >> __btod_div_common
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  _btod_emul (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_emul))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_emul ⇒ _e2e
  [Calls]
  - >> __btod_mult_common
  - >> _e2e
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  __btod_mult_common (Thumb, 580 bytes, Stack size 16 bytes, btod.o(CL$$btod_mult_common))
  [Stack]

  - Max Depth = 16
  - Call Chain = __btod_mult_common
  [Called By]
  - >> _btod_emul

  __ARM_fpclassify (Thumb, 40 bytes, Stack size 0 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Called By]

  - >> _printf_fp_dec_real

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  sqrt (Thumb, 78 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  _get_lc_numeric (Thumb, 44 bytes, Stack size 8 bytes, lc_numeric_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_numeric
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_numeric_2

  _get_lc_ctype (Thumb, 44 bytes, Stack size 8 bytes, lc_ctype_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_ctype
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_ctype_2
  [Address Reference Count : 1]
  - rt_ctype_table.o(.text)

  __aeabi_dadd (Thumb, 0 bytes, Stack size 16 bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)

  _dadd (Thumb, 332 bytes, Stack size 16 bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)
  [Calls]

  - >> _dsub1
  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> CTP_Scan
  - >> TP_Adjust

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt))
  [Called By]

  - >> CTP_Scan

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu))
  [Called By]

  - >> TP_Adjust

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmple
  [Called By]
  - >> TP_Adjust

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __aeabi_dmul (Thumb, 0 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dmul
  [Called By]
  - >> CTP_Scan

  _dmul (Thumb, 332 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _dmul
  - >> _dcmple
  - >> _dfixu
  - >> _dsub
  - >> _dadd
  - >> _dsqrt

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _f2d
  - >> _dmul
  - >> _dadd

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> TP_Adjust

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  __aeabi_drsub (Thumb, 0 bytes, Stack size 8 bytes, daddsub_clz.o(x$fpl$drsb))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_drsub
  [Called By]
  - >> CTP_Scan

  _drsb (Thumb, 22 bytes, Stack size 8 bytes, daddsub_clz.o(x$fpl$drsb), UNUSED)
  [Calls]

  - >> _dsub1
  - >> _dadd1

  _dsqrt (Thumb, 456 bytes, Stack size 24 bytes, dsqrt_noumaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> sqrt

  __aeabi_dsub (Thumb, 0 bytes, Stack size 32 bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)

  _dsub (Thumb, 464 bytes, Stack size 32 bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)
  [Calls]

  - >> _dadd1
  - >> __fpl_dnaninf

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> TP_Adjust

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __aeabi_fadd (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fadd
  [Called By]
  - >> TP_Scan

  _fadd (Thumb, 196 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Calls]

  - >> _fsub1
  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __aeabi_fdiv (Thumb, 0 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fdiv
  [Called By]
  - >> TP_Adjust

  _fdiv (Thumb, 384 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __aeabi_f2iz (Thumb, 0 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2iz
  [Called By]
  - >> TP_Adjust

  _ffix (Thumb, 54 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_f2uiz (Thumb, 0 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2uiz
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  _ffixu (Thumb, 62 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_i2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt))
  [Called By]

  - >> TP_Adjust
  - >> TP_Scan

  _fflt (Thumb, 48 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt), UNUSED)

  __aeabi_ui2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu))
  [Called By]

  - >> TP_Adjust
  - >> TP_Scan

  _ffltu (Thumb, 38 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu), UNUSED)

  __aeabi_fmul (Thumb, 0 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  _fmul (Thumb, 258 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _ffixu
  - >> _ffix
  - >> _fdiv
  - >> _fsub
  - >> _fadd
  - >> _f2d

  __fpl_fretinf (Thumb, 10 bytes, Stack size 0 bytes, fretinf.o(x$fpl$fretinf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _fdiv
  - >> _fadd

  __aeabi_fsub (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fsub
  [Called By]
  - >> TP_Adjust

  _fsub (Thumb, 234 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Calls]

  - >> _fadd1
  - >> __fpl_fnaninf

  _printf_fp_dec (Thumb, 4 bytes, Stack size 0 bytes, printf1.o(x$fpl$printf1))
  [Stack]

  - Max Depth = 320
  - Call Chain = _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec_real
  [Called By]
  - >> _printf_g
  - >> _printf_e
  - >> _printf_f

  ### Local Symbols

  SetSysClockTo72 (Thumb, 212 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  TI4_Config (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 122 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 108 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  mem_cpy (Thumb, 26 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> dir_register
  - >> gen_numname
  - >> f_write
  - >> f_unlink
  - >> f_setlabel
  - >> f_rename
  - >> f_read
  - >> f_mkfs
  - >> f_mkdir
  - >> f_getlabel

  mem_set (Thumb, 20 bytes, Stack size 12 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> create_name
  - >> dir_remove
  - >> dir_register
  - >> dir_next
  - >> sync_fs
  - >> f_setlabel
  - >> f_mkfs
  - >> f_mkdir

  mem_cmp (Thumb, 38 bytes, Stack size 20 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> dir_find

  chk_chr (Thumb, 20 bytes, Stack size 0 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> create_name
  - >> f_setlabel

  sync_window (Thumb, 76 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> disk_write
  [Called By]
  - >> dir_next
  - >> sync_fs
  - >> move_window
  - >> f_mkdir

  move_window (Thumb, 50 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> sync_window
  - >> disk_read
  [Called By]
  - >> f_sync
  - >> put_fat
  - >> get_fat
  - >> find_volume
  - >> check_fs
  - >> dir_remove
  - >> dir_register
  - >> dir_read
  - >> dir_find
  - >> dir_alloc
  - >> f_rename
  - >> f_open
  - >> f_getlabel
  - >> f_getfree

  sync_fs (Thumb, 200 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> sync_window
  - >> mem_set
  - >> disk_ioctl
  - >> disk_write
  [Called By]
  - >> f_utime
  - >> f_chmod
  - >> f_sync
  - >> f_unlink
  - >> f_setlabel
  - >> f_rename
  - >> f_mkdir

  remove_chain (Thumb, 108 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_truncate
  - >> f_unlink
  - >> f_open
  - >> f_mkdir

  create_chain (Thumb, 214 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> put_fat
  - >> get_fat
  [Called By]
  - >> dir_next
  - >> f_write
  - >> f_mkdir
  - >> f_lseek

  clmt_clust (Thumb, 50 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> f_write
  - >> f_read
  - >> f_lseek

  dir_sdi (Thumb, 158 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> clust2sect
  [Called By]
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> dir_find
  - >> dir_alloc
  - >> f_unlink
  - >> f_setlabel
  - >> f_readdir
  - >> f_opendir
  - >> f_getlabel

  dir_next (Thumb, 270 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> clust2sect
  - >> create_chain
  - >> sync_window
  - >> mem_set
  [Called By]
  - >> dir_remove
  - >> dir_register
  - >> dir_read
  - >> dir_find
  - >> dir_alloc
  - >> f_readdir

  dir_alloc (Thumb, 92 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> dir_next
  - >> dir_sdi
  - >> move_window
  [Called By]
  - >> dir_register
  - >> f_setlabel

  ld_clust (Thumb, 32 bytes, Stack size 8 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> follow_path
  - >> f_unlink
  - >> f_rename
  - >> f_opendir
  - >> f_open

  st_clust (Thumb, 16 bytes, Stack size 0 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> f_sync
  - >> f_rename
  - >> f_open
  - >> f_mkdir

  cmp_lfn (Thumb, 138 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> ff_wtoupper
  [Called By]
  - >> dir_find

  pick_lfn (Thumb, 112 bytes, Stack size 20 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> dir_read

  fit_lfn (Thumb, 122 bytes, Stack size 20 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> dir_register

  gen_numname (Thumb, 192 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> mem_cpy
  [Called By]
  - >> dir_register

  sum_sfn (Thumb, 32 bytes, Stack size 12 bytes, ff.o(.text), UNUSED)
  [Called By]

  - >> dir_register
  - >> dir_read
  - >> dir_find

  dir_find (Thumb, 222 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> sum_sfn
  - >> cmp_lfn
  - >> dir_next
  - >> dir_sdi
  - >> move_window
  - >> mem_cmp
  [Called By]
  - >> follow_path
  - >> dir_register

  dir_read (Thumb, 196 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> sum_sfn
  - >> pick_lfn
  - >> dir_next
  - >> move_window
  [Called By]
  - >> f_unlink
  - >> f_setlabel
  - >> f_readdir
  - >> f_getlabel

  dir_register (Thumb, 308 bytes, Stack size 48 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> dir_find
  - >> sum_sfn
  - >> gen_numname
  - >> fit_lfn
  - >> dir_alloc
  - >> dir_next
  - >> dir_sdi
  - >> move_window
  - >> mem_set
  - >> mem_cpy
  [Called By]
  - >> f_rename
  - >> f_open
  - >> f_mkdir

  dir_remove (Thumb, 106 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> dir_next
  - >> dir_sdi
  - >> move_window
  - >> mem_set
  [Called By]
  - >> f_unlink
  - >> f_rename

  get_fileinfo (Thumb, 268 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> ff_convert
  [Called By]
  - >> f_stat
  - >> f_readdir

  create_name (Thumb, 602 bytes, Stack size 56 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> ff_wtoupper
  - >> ff_convert
  - >> chk_chr
  - >> mem_set
  [Called By]
  - >> follow_path

  follow_path (Thumb, 144 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> create_name
  - >> dir_find
  - >> ld_clust
  - >> dir_sdi
  [Called By]
  - >> f_utime
  - >> f_chmod
  - >> f_stat
  - >> f_unlink
  - >> f_rename
  - >> f_opendir
  - >> f_open
  - >> f_mkdir

  get_ldnumber (Thumb, 74 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = get_ldnumber
  [Called By]
  - >> f_mount
  - >> find_volume
  - >> f_rename
  - >> f_mkfs

  check_fs (Thumb, 140 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> move_window
  [Called By]
  - >> find_volume

  find_volume (Thumb, 916 bytes, Stack size 80 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 272
  - Call Chain = find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> check_fs
  - >> get_ldnumber
  - >> move_window
  - >> disk_status
  - >> disk_initialize
  [Called By]
  - >> f_mount
  - >> f_utime
  - >> f_chmod
  - >> f_stat
  - >> f_unlink
  - >> f_setlabel
  - >> f_rename
  - >> f_opendir
  - >> f_open
  - >> f_mkdir
  - >> f_getlabel
  - >> f_getfree

  validate (Thumb, 54 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> disk_status
  [Called By]
  - >> f_truncate
  - >> f_sync
  - >> f_write
  - >> f_readdir
  - >> f_read
  - >> f_lseek
  - >> f_closedir
  - >> f_close

  putc_bfd (Thumb, 68 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_write
  [Called By]
  - >> f_printf
  - >> f_puts
  - >> f_putc

  _dadd1 (Thumb, 0 bytes, Stack size unknown bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)
  [Called By]

  - >> _dsub
  - >> _drsb

  _dsub1 (Thumb, 0 bytes, Stack size unknown bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)
  [Called By]

  - >> _drsb
  - >> _dadd

  _fadd1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Called By]

  - >> _fsub

  _fsub1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Called By]

  - >> _fadd

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  _fp_digits (Thumb, 426 bytes, Stack size 96 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  - >> _btod_d2e
  - >> _btod_etento
  - >> _ll_udiv10
  [Called By]
  - >> _printf_fp_dec_real

  ### Undefined Global Symbols