#

##

##

    µVision Build Log
    Project:
    F:\starm\GPIO_LED(2014.12.19)\project.uvproj
    Project File Date:  01/06/2015

    Output:
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12072 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.261V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12072 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.261V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12072 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12072 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12108 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12112 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12112 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12136 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12136 RO-data=420 RW-data=44 ZI-data=1716
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    user\main.c(236): error:  #18: expected a ")"
    user\main.c(255): warning:  #12-D: parsing restarts here after previous syntax error
    user\main.c(255): error:  #127: expected a statement
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    Target not created
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12144 RO-data=420 RW-data=48 ZI-data=1712
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12144 RO-data=420 RW-data=48 ZI-data=1712
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12144 RO-data=420 RW-data=48 ZI-data=1712
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12144 RO-data=420 RW-data=48 ZI-data=1712
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12144 RO-data=420 RW-data=48 ZI-data=1712
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Rebuild target 'project'
    compiling stm32f2xx_usart.c...
    compiling misc.c...
    compiling stm32f2xx_crc.c...
    compiling stm32f2xx_gpio.c...
    compiling stm32f2xx_rcc.c...
    compiling stm32f2xx_syscfg.c...
    compiling stm32f2xx_fsmc.c...
    compiling stm32f2xx_tim.c...
    compiling stm32f2xx_adc.c...
    compiling stm32f2xx_dma.c...
    compiling core_cm3.c...
    compiling system_stm32f2xx.c...
    compiling main.c...
    compiling stm32f2xx_it.c...
    assembling startup_stm32f2xx.s...
    linking...
    Program Size: Code=12144 RO-data=420 RW-data=48 ZI-data=1712
    FromELF: creating hex file...
    ".\Obj\project.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\starm\\GPIO_LED(2014.12.19)\\Obj\\project.AXF"
    * JLink Info: Device "STM32F207VG" selected (1024 KB flash, 64 KB RAM).
    Set JLink Project File to "F:\starm\GPIO_LED(2014.12.19)\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.50j, compiled Jun 26 2012 09:19:07
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999994
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r2p0, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F207VG
    VTarget = 3.267V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...