**Relative Code Domain Error (RCDE) Measurement**

1. Manual measurement from MXA for Code EVM for every code.
2. Convert the % EVM value into a factor
3. Manual measurement from MXA of Code Domain Power for every code.
4. Convert log dB of CDP into its corresponding factor
5. Calculate using this formula

